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Road tunnel and service tunnel structures
Technical approval (TA) requirements in this section shall be followed for the following:

1) road tunnel structures;
2) service tunnels where the internal diameter is greater than 2 m; and,
3) major tunnelling or building operations within the zone of influence of an existing road tunnel.

This section shall be read in conjunction with Sections 1, 2 and 6, and in the case of cut-and-over
construction and for tunnel portals and road decks, the relevant parts of Section 3.

The requirements of the Tunnel Design and Safety Consultation Group shall be complied with.

The TA requirements within this document shall not apply to service tunnels where the internal
diameter is 2 m or less.

For service tunnels where the internal diameter is 2 m or less requirements of CD 622 [Ref 11.N] shall
apply.

Scope of TA requirements for tunnels

In addition to clause 1.1, the procedures described in this Section shall be applied to:

1) the design and execution of new road tunnels, tunnel services buildings and service tunnels;

2) the assessment of existing tunnels that are subject to the effects of new temporary or permanent
construction above or adjacent to the tunnel structure; and,

3) the refurbishment and strengthening of existing road tunnels.

Category

In addition to clauses 2.20 to 2.26, proposals for the design or assessment of road tunnel structures
and service tunnels shall be in category 3.




